**Software Upgrade**

1.Prepare to sofeware files under the root directory in U disk:

One of the files is CtvUpgrade.bin,

The file is following:



2. The system is powered down (Turn off the power switch or unplug the power

plug)

3. Connect with U disk to USB2.0 interface.

4. System on power (Turn on the power switch or connect to the power supply

plug )

5. After about three seconds, you can see the power indicator light flashes, which

means the upgrade is on.

If ten seconds later, there are no indicato lright flashes, you need to check

whether the U disk files exit and the name is right or not. Make sure it and skip

to step2.

6. It needs about 3 minutes to complete upgrading, when the upgrade is

completed, the system will restart automatically. If the picture is standard screen

which is designed for factory automation, which means the upgrade is

successful.

7. After upgrading successfully, unplug the U disc.

8. You will enter the new system after powering and powering o n.